液氮MCT检测器参数：

MCT detector, medium band

Liquid N2 cooled

Spectral range: 12,000-600cm-1

D\*: >2x10\*\*10cm Hz½/W

Hold time: typically 8h

Integrated amplifier and digitizing electronics